Dehumidifiers Key Efficiency Criteria

Qualified models meet all ENERGY STAR requirements as listed in the Version 3.0 ENERGY STAR Program Requirements for Dehumidifiers that are effective as of October 1, 2012.

|  |  |  |
| --- | --- | --- |
| **Equipment** | **Specification** | |
| **Product Capacity (pints/day)** | **Energy Factor Under Test Conditions (L/kWh)** |
| Dehumidifiers | < 75 | ≥ 1.85 |
| 75 to ≤ 185 | ≥ 2.80 |